LabelWriter

Project	LabelWriter
Description	We have a label writer, get it working on any platform!
Status	Active
Contact	metalgamer
Participants:

Hardware

We have a Dymo LabelManager Wireless PnP.

Installation

Linux

It prints, but the data is not correctly positioned, so it is practically unusable! If you got any clues on how to get a correct configuration, please let me know!

Archlinux

First we need to install the dymo-cups-drives package from the AUR.

Next we need to install the usb_modeswitch package using pacman.

Now create the file with the following content:

<sxh> # Dymo LabelManager PnP

DefaultVendor= 0x0922 DefaultProduct=0x1007

TargetVendor= 0x0922 TargetProduct= 0x1008

MessageEndpoint= 0x01 ResponseEndpoint=0x01

MessageContent="1b5a01" </sxh>

Now run as root.

Download the following PPD file to

Now add the printer to CUPS and you're should be good to go.