Meshtastic

Name	Meshtastic
Description

How it works

Meshtastic utilizes LoRa, a long-range radio protocol, which is widely accessible in most regions without the need for additional licenses or certifications, unlike ham radio operations.

These radios are designed to rebroadcast messages they receive, forming a mesh network. This setup ensures that every group member, including those at the furthest distance, can receive messages.

Here I document experiences and channel information about the nodes we use in Luxembourg.

Additionally, Meshtastic radios can be paired with a single phone, allowing friends and family to send messages directly to your specific radio. It's important to note that each device is capable of supporting a connection from only one user at a time. |

Status	Running
Contact	orimpe
Participants
Repository